### RAS Console
Source | Destination | Protocols | Ports | Description
RAS Console | RAS Reporting | TCP | 30008 | RAS Console is connected to primary RAS Publishing Agent which communicates with RAS Reporting (installed on the same host as SSRS). SSRS talks to SQL via TCP 1433 (or dynamic if 1433 is not established in the settings).
| HALB | TCP, UDP | 31006 | Used for configuration.
| Parallels Client | TCP | 50005 | Shadowing from the RAS Console in case of direct network connection.
| RAS RD Session Host Agent RAS Guest Agent RAS Remote PC Agent RAS Publishing Agent RAS Secure Client Gateway RAS Enrollment Server | TCP | 135, 445, 49179 | Remote install push/takeover of software.
| RAS RD Session Host Agent | UDP, TCP | 30004 | Used for the "Check Agent" task. Used to manage components.
| RAS Guest Agent | TCP UDP | 30010 30009 | Used for the "Check Agent" task. Used to manage components.
| RAS Remote PC Agent | UDP, TCP | 30004 | Used for the "Check Agent" task. Used to manage components.
| RAS VDI Agent | UDP, TCP | 30006 | Used for the "Check Agent" task. Used to manage component.
| MFA Server(s) | TCP, UDP | 8080, 80, 1812, 1813 | Deepnet / Safenet / Radius
| www.turbo.net | TCP | 80, 443 | Note: Turbo.net public repository integration with the RAS console has been deprecated in Parallels RAS 18, but existing Turbo.net applications already configured on the RD Session Hosts will remain available. The ports are used to obtain app categories and available app metadata for Turbo public repository.
| RAS Performance Monitor | TCP | 3000 | Performance Dashboard in the Monitoring category (Grafana connection).
| RAS Publishing Agent | TCP | 20002, 20001 30020 | Communication with Publishing Agent and redundancy. 30020 - remote agent pushing.
| RAS Enrollment Server | TCP, UDP | 30030 | Used for the "Check Agent" task. Used to manage components and for troubleshooting.
| Wyse Broker | UDP | 1234 (outbound only) 68 (inbound only) | Wyse broker discovery request broadcast packet (V_WYSEBCAST). Wyse broker discovery reply packet (V_WYSETEST).