### RAS VDI Agent
Source | Destination | Protocols | Ports | Description
RAS VDI Agent | RAS Publishing Agent | TCP | 20003 | Publishing Agent communication port.
| RAS Guest Agent | TCP | 135, 49152-65535 | WMI ports. Port 135 is a standard RPC port. WMI also uses a randomly assigned port from the 49152-65535 range in Windows Vista, 2008 and above.
| RAS Performance Monitor | TCP | 8086 | Agent (Telegraf service) sends collected performance data to InfluxDB - applicable to Hyper-V only.
| Hyper-V | TCP | 135, 49152-65535 | WMI ports. Port 135 is a standard RPC port. WMI also uses a randomly assigned port from the 49152-65535 range in Windows Vista, 2008 and above.
| Nutanix | TCP | 9440 | Nutanix REST port
| VMWare | TCP | 443 | Taken from Required Ports for vCenter Server . This port is also used for the following services: - WS-Management (also requires port 80 to be open) - Third-party network management client connections to vCenter Server - Third-party network management clients access to hosts