### Changing the HALB Appliance Password To change the HALB appliance password: Boot the appliance (virtual machine). Press the <ALT> – <F1> key combination. A login prompt should be displayed. Type in the following credentials: login: `root` password: `Pa$$w0rd` (note that "0" is zero, not the letter "O"). Once logged in, execute the password changing command and type a new password. Upon completion, you may log in to the HALB device with the new password.